The State Configurable Timer (SCT) allows a wide variety of timing, counting, output

modulation, and input capture operations.

P1.6 connected to tsop38238

Selects an input source for SCT0 input